0 50 100 150 0

5

10

15

20

25

30

35

6.25 5 4 3 2

number of nodes

Megaflops per node

LU: Predicted Total Performance for Constant Memory Use